{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A"]
[]
[]
[]
[]
["","","","","","2MXM40A2V1B","2MXM50A2V1B","2MXM68A2V1B"]
["Dimensions","Unité","","Hauteur","mm","","552","734"]
["","","","Largeur","mm","","852","974"]
["","","","Profondeur","mm","","350","408"]
["Poids","Unité","","","kg","","41","60"]
["Compresseur","Type","","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîch.","Temp. ambiante","Min.","°CBS","","-10","-10"]
["","","","Max.","°CBS","","46","46"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","48","48"]
["","Chauffage","","Nom.","dBA","","50","48"]
["Réfrigérant","Type","","","","","R-32","R-32"]
["","Charge","","","kg","","1.15","2.00"]
["","PRP","","","","","675","675"]
["Raccords de tuyauterie","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","","15","15"]
["","","UI - UI","Max.","m","","7.5","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","","30","50"]
["Accessoires standard","Manuel d'installation","","","","","1","1"]
["","Sachet de vis","","","","","1","1"]
["","Bouchon d'évacuation","","","","","1","1"]
["","Réducteur","","","","","1","1"]
["Power supply","Phase","","","","","1~","1~"]
["","Fréquence","","","Hz","","50","50"]
["","Tension","","","V","","220-240","220-240"]
["Remarques","","","","","(1) - Par pièce","(1) - Par pièce","(1) - Par pièce"]
["","","","","","(2) - Pour combinaison avec CVXM-A, FVXM-A - la longueur maximale de tuyauterie est 30 m.","(2) - Pour combinaison avec CVXM-A, FVXM-A - la longueur maximale de tuyauterie est 30 m.","(2) - Pour combinaison avec CVXM-A, FVXM-A - la longueur maximale de tuyauterie est 30 m."]
["","","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(5) - Contient des gaz à effet de serre fluorés.","(5) - Contient des gaz à effet de serre fluorés.","(5) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","552"]
["","","","Largeur","mm","852"]
["","","","Profondeur","mm","350"]
["Poids","Unité","","","kg","36"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10"]
["","","","Max.","°CBS","46"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","46"]
["","Chauffage","","Nom.","dBA","48"]
["Réfrigérant","Type","","","","R-32"]
["","Charge","","","kg","0.88"]
["","Charge","","","tCO2Eq","0.60"]
["Réfrigérant","PRP","","","","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20 (1)"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 20 m)"]
["","Dénivelé","UI - UE","Max.","m","15"]
["","","UI - UI","Max.","m","7.5"]
["Raccords de tuyauterie","Longueur totale de tuyauterie","Système","Réel","m","30"]
["Accessoires standard","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50"]
["","Alimentation électrique-=-Tension","","Tension","","220-240"]
["Accessoires standard","Bouchon d’évacuation","","","","","","3"]