{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA50A2VEB","ADEA100A2VEB"]
["Ventilateur","Pression statique externe","","Haute","Pa","","150"]
["Caisson","Couleur","","","","","Non peinte (galvanisée)"]
["Caisson","Matériau","","","","","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","","245"]
["","","","Largeur","mm","","1400"]
["","","","Profondeur","mm","","800"]
["Poids","Unité","","","kg","","46"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","29"]
["Ventilateur","Débit d'air","Rafraîchissement","Moyen","m³/min","","26"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","23"]
["","","Chauffage","Haut","m³/min","","29"]
["Ventilateur","Débit d'air","Chauffage","Moyen","m³/min","","26"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","23"]
["","Pression statique externe","","Nom.","Pa","","40"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","34"]
["Niveau de pression sonore","Rafraîchissement","","Moyen","dBA","","32"]
["Niveau de pression sonore","Rafraîchissement","","Bas","dBA","","30"]
["","Chauffage","","Haut","dBA","","36"]
["","","","Moyen","dBA","","33"]
["","","","Bas","dBA","","30"]
["Raccords de tuyauterie","Liquide","","DE","mm","","9.52"]
["Raccords de tuyauterie","Gaz","","DE","mm","","15.9"]
["Raccords de tuyauterie","Évacuation","","","","","VP20 (I.D. 20/O.D. 26)"]
["Hauteur manométrique","mm","","","","","625"]
["Systèmes de contrôle","Infrared remote control","","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessoires standard","Installation manual","","","","","1"]
["","Washer for hanger bracket","","","","","8"]
["","Operation manual","","","","","1"]
["","Clamps","","","","","4"]
["","Drain hose","","","","","1"]
["","Insulation for fitting","","","","","2"]
["","Metal clamp for drain hose","","","","","1"]
["","Screws","","","","","40"]
["","Sealing pads","","","","","5"]
["Alimentation électrique","Phase","","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","","50"]
["","Alimentation électrique-=-Tension","","Tension","","","220-240/220"]
["Accessoires standard","AAA dry-cell batteries","","","","3"]