{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":89,"n_cols":8,"rows_kept":89,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M"]
[]
[]
[]
[]
["","","","","","FTXP50M2V1B","FTXP25M5V1B","FTXP60M2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","40","40"]
["","","","Moyen","dBA","","34","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["","","","Bas","dBA","","28","32"]
["","Rafraîchissement","","Moyen","dBA","","33","41"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19","30"]
["","","","Bas","dBA","","26","36"]
["","","","Haut","dBA","","40","45"]
["Accessoires standard","Manuel d'installation","","","","","1","1"]
["","Manuel d’utilisation","","","","","1","1"]
["","Télécommande infrarouge","","","","","1","1"]
["","Piles sèches AAA","","","","","2","2"]
["","Support de télécommande","","","","","1","1"]
["","Plaque de montage","","","","","1","1"]
["","Filtre désodorisant à apatite de titane","","","","","2","1"]
["","Vis de fixation d'unité intérieure","","","","","2","2"]
["Systèmes de contrôle","Wired remote control","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","ARC480A53","ARC480A53"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35","6.35"]
["","Gaz","","DE","mm","","9.50","12.7"]
["","Evacuation","","","","","18","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.020","0.032"]
["","Chauffage","","Nom.","kW","","0.023","0.035"]
["Sound power level","Rafraîchissement","","","dBA","","55","60"]
["","Chauffage","","","dBA","","55","62"]
["Dimensions","Unité","","Largeur","mm","","770","990"]
["","","","Profondeur","mm","","225","263"]
["","","","Hauteur","mm","","286","295"]
["Caisson","Couleur","","","","","Blanc","Blanc"]
["Poids","Unité","","","kg","","8.50","13.5"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","","10.4","17.9"]
["","","","Moyen","m³/min","","8.1","15.3"]
["","","","Bas","m³/min","","6.4","12.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","5.2","11.0"]
["","","Rafraîchissement","Bas","m³/min","","5.8","11.8"]
["","","","Moyen","m³/min","","7.7","14.4"]
["","","","Haut","m³/min","","9.7","16.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.2","9.2"]
["Power supply","Phase","","","","","1~","1~"]
["","Nom","","","","","","V1"]
["","Fréquence","","","Hz","","50","50"]
["","Tension","","","V","","220-240","220-240"]
["Raccords de tuyauterie","Évacuation","","","","18"]
["Raccords de tuyauterie","Piping connections-=-Gas-=-OD","","","mm","12.7"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Liquide-=-DE","","","mm","6.35"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement-=-Bas","","","dBA","34"]
["","Niveau de pression sonore-=-Rafraîchissement-=-Haut","","","dBA","43"]
["Unité","kg","","","","13.5"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage-=-Faible niveau sonore de fonctionnement","","","dBA","30"]
["","Niveau de pression sonore-=-Chauffage-=-Haut","","","dBA","42"]
["","Niveau de pression sonore-=-Chauffage-=-Bas","","","dBA","33"]
["Rafraîchissement","dBA","","","","59"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement","","","dBA","27"]
["Caisson","Couleur","","","","Blanc"]
["Ventilateur","Débit d'air","","Ventilateur-=-Débit d'air-=-Chauffage-=-Haut","m³/min","17.3"]
["Dimensions","Dimensions-=-Unité-=-Profondeur","","","mm","263"]
["Ventilateur","Débit d'air","","Ventilateur-=-Débit d'air-=-Chauffage-=-Bas","m³/min","11.8"]
["Dimensions","Dimensions-=-Unité-=-Largeur","","","mm","990"]
["","Hauteur","","","mm","295"]
["Systèmes de contrôle","Infrared remote control","","","","ARC480A53"]
["Chauffage","dBA","","","","61"]
["Puissance absorbée","Nom.","","","kW","0.029"]
["","Nom.","","","kW","0.032"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage-=-Moyen","","","dBA","38"]
["Niveau de pression sonore","Sound pressure level-=-Cooling-=-Medium","","","dBA","39"]
["Ventilateur","Débit d'air","","Ventilateur-=-Débit d'air-=-Chauffage-=-Faible niveau sonore de fonctionnement","m³/min","10.4"]
["","","","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement","m³/min","8.3"]
["Ventilateur","Débit d'air","","Fan-=-Air flow rate-=-Cooling-=-Medium","m³/min","14.0"]
["","","","Fan-=-Air flow rate-=-Heating-=-Medium","m³/min","14.4"]
["Accessoires standard","Installation manual","","","","Installation manual"]
["","AAA dry-cell batteries","","","","AAA dry-cell batteries"]
["","Operation manual","","","","Operation manual"]
["","Titanium apatite deodorizing filter","","","","Titanium apatite deodorizing filter"]
["","Silver particle filter","","","","Silver particle filter"]
["","Indoor unit fixing screws","","","","Indoor unit fixing screws"]
["","Infrared remote control","","","","Infrared remote control"]
["","Mounting plate","","","","Mounting plate"]
["","Remote control holder","","","","Remote control holder"]
["Alimentation électrique","Alimentation électrique-=-Fréquence","","","","50"]
["","Phase","","","","1~"]
["","Alimentation électrique-=-Tension","","","","220-240"]
["","Nom","","","","V1"]
["Accessoires standard","Filtre à particules argent","","","","","","1"]