{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP35M5V1B9"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","40"]
["","","","Moyen","dBA","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","","","Bas","dBA","29"]
["","Rafraîchissement","","Moyen","dBA","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","20"]
["","","","Bas","dBA","27"]
["","","","Haut","dBA","43"]
["Systèmes de contrôle","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A53"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Evacuation","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.032"]
["","Chauffage","","Nom.","kW","0.032"]
["Sound power level","Rafraîchissement","","","dBA","58"]
["","Chauffage","","","dBA","58"]
["Dimensions","Unité","","Largeur","mm","770"]
["","","","Profondeur","mm","225"]
["","","","Hauteur","mm","286"]
["Caisson","Couleur","","","","Blanc"]
["Poids","Unité","","","kg","9.00"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","11.5"]
["","","","Moyen","m³/min","9.0"]
["","","","Bas","m³/min","7.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3"]
["","","Rafraîchissement","Bas","m³/min","6.3"]
["","","","Moyen","m³/min","8.3"]
["","","","Haut","m³/min","11.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]