{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Puissance absorbée","Puissance absorbée-=-Chauffage","","Puissance absorbée-=-Chauffage-=-Nom.-=-kW","kW","0.03","0.030","0.030"]
["","Puissance absorbée-=-Rafraîchissement","","Puissance absorbée-=-Rafraîchissement-=-Nom.-=-kW","kW","0.03","0.030","0.030"]
["Niveau de puissance sonore","Niveau de puissance sonore-=-Chauffage-=-dBA","","","dBA","56","57","59"]
["Systèmes de contrôle","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Rafraîchissement","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Haut-=-m³/min","m³/min","10.7","12.1","15.0"]
["","","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Haut-=-m³/min","m³/min","11.7","13.3","14.4"]
["","","","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Bas-=-m³/min","m³/min","5.3","5.6","6.6"]
["","","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Bas-=-m³/min","m³/min","6.7","6.9","7.7"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Largeur-=-mm","mm","798","798","798"]
["","","","Dimensions-=-Unité-=-Hauteur-=-mm","mm","295","295","295"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Rafraîchissement","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Nom.-=-m³/min","m³/min","7.5","8.4","9.2"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Profondeur-=-mm","mm","372","372","372"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Faible niveau sonore de fonctionnement-=-dBA","dBA","19","19","24"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Faible niveau sonore de fonctionnement-=-m³/min","m³/min","4.8","4.8","5.9"]
["","","Ventilateur-=-Débit d'air-=-Rafraîchissement","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement-=-m³/min","m³/min","4","4.0","4.6"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Haut-=-dBA","dBA","38","42","47"]
["Poids","Unité","","","kg","15","15","15"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Liquide","","Raccords de tuyauterie-=-Liquide-=-DE-=-mm","mm","6.35","6.35","6.35"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Bas-=-dBA","dBA","26","27","30"]
["Raccords de tuyauterie","Gaz","","DE","mm","9.5","9.5","9.5"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement-=-dBA","dBA","19","19","23"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Bas-=-dBA","dBA","28","29","31"]
["Niveau de puissance sonore","Niveau de puissance sonore-=-Rafraîchissement-=-dBA","","","dBA","54","57","60"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Haut-=-dBA","dBA","39","42","44"]
["","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Nom.-=-dBA","dBA","33","35","38"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Nom.-=-m³/min","m³/min","8.6","9.2","10.7"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Nom.-=-dBA","dBA","35","36","38"]
["Accessoires standard","Wireless remote control","","","","1","1","1"]
["","Photocatalytic air purifying and deodorising filter","","","","1","1","1"]
["","Dry batteries","","","","2","2","2"]
["","Indoor unit fixing screws","","","","3","3","3"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Alimentation électrique","Alimentation électrique-=-Nom","","","","V1","V1","V1"]
["","Alimentation électrique-=-Phase","","","","1~","1~","1~"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240","220-240","220-240"]
["","Alimentation électrique-=-Fréquence","","Alimentation électrique-=-Fréquence-=-Hz","","50","50","50"]
["Remarques","","","","","(1) - 230 V","(1) - Arrière de l'échangeur de chaleur","(1) - Arrière de l'échangeur de chaleur"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - Avant de l'échangeur de chaleur","(3) - 230 V"]
["","","","","","(4) - Arrière de l'échangeur de chaleur","(4) - 230 V","(4) - Avant de l'échangeur de chaleur"]
["","","","","","(5) - Avant de l'échangeur de chaleur","(5) - 240V","(5) - 240V"]