{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG35K2V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)"]
["","Chauffage","","Nom.","kW","0.024 (1) (2) (3), 0.024 (1) (2) (3), 0.024 (1) (2) (3)"]
["Caisson","Couleur","","","","Blanc frais (6.5Y 9.5/0.5)"]
["Dimensions","Unité","","Hauteur","mm","600"]
["","","","Largeur","mm","950"]
["","","","Profondeur","mm","215"]
["Poids","Unité","","","kg","22.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","9.1"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","5.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5"]
["","","Chauffage","Haut","m³/min","10.2"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.0"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","55"]
["","Chauffage","","","dBA","56"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","39"]
["","Refroidissement","","Moyen","dBA","33"]
["","","","Bas","dBA","27"]
["","","","Faible niveau sonore de fonctionnement","dBA","24"]
["","Chauffage","","Haut","dBA","40"]
["","","","Moyen","dBA","33"]
["","","","Bas","dBA","27"]
["","","","Faible niveau sonore de fonctionnement","dBA","23"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Évacuation","","","","18"]
["Systèmes de contrôle","Infrared remote control","","","","ARC466A2"]
["Accessoires standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Installation plate","","","","1"]
["","Thermal insulation (thermal insulation tube)","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Drain hose","","","","1"]
["","Remote control holder","","","","1"]
["Alimentation électrique","Nom","","","","V1"]
["","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50"]
["","Alimentation électrique-=-Tension","","Tension","","220-240"]
["Remarques","","","","","(1) - 220V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240V"]