{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":7,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","","FXFA100A2VEB","FXFA125A2VEB (Archived)"]
["Réfrigérant","Type","","","","","R-32"]
["Réfrigérant","PRP","","","","","675.0"]
["Caisson","Matériau","","","","","Tôle en acier galvanisé"]
["Dimensions","Unité","","Largeur","mm","","840"]
["","","","Dimensions-=-Unité-=-Hauteur-=-mm @","mm","","288"]
["","","","Profondeur","mm","","840"]
["Poids","Unité","","","kg","","26"]
["Puissance frigorifique","Puissance totale","","Cooling capacity-=-Total capacity-=-At high fan speed-=-kW @","kW","","14.00"]
["Puissance calorifique","Puissance totale","","Heating capacity-=-Total capacity-=-At high fan speed-=-kW @","kW","","16.00"]
["Ventilateur","Débit d'air - 50Hz","Rafraîchissement","À grande vitesse de ventilation","m³/min","","33.0"]
["","","","À petite vitesse de ventilation","m³/min","","20.6"]
["Puissance absorbée - 50Hz","Rafraîchissement","","Power input - 50Hz-=-Cooling-=-At high fan speed-=-kW @","kW","","0.103"]
["","Chauffage","","Power input - 50Hz-=-Heating-=-At high fan speed-=-kW @","kW","","0.103"]
["Niveau de pression sonore","Rafraîchissement","","Sound pressure level-=-Cooling-=-At high fan speed-=-dBA @","dBA","","45.0"]
["","","","Sound pressure level-=-Cooling-=-At medium fan speed-=-dBA @","dBA","","41.0"]
["","Chauffage","","Sound pressure level-=-Heating-=-At high fan speed-=-dBA @","dBA","","45.0"]
["","","","Sound pressure level-=-Heating-=-At medium fan speed-=-dBA @","dBA","","41.0"]
["","","","Sound pressure level-=-Cooling-=-At low fan speed-=-dBA @","dBA","","36.0"]
["Sound power level","Rafraîchissement","","À grande vitesse de ventilation","dBA","","61.0"]
["Filtre à air","Type","","","","","Tamis en résine"]
["Panneau décoratif","Dimensions","","Largeur","mm","","950"]
["Niveau de pression sonore","Chauffage","","Sound pressure level-=-Heating-=-At low fan speed-=-dBA @","dBA","","36.0"]
["Raccords de tuyauterie","Évacuation","","","","","VP25 (O.D. 32 / I.D. 25)"]
["Panneau décoratif","Modèle","","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensions","","Hauteur","mm","","65"]
["Façade 2","Façade 2-=-Poids-=-kg","","","kg","","10.3"]
["Panneau décoratif","Dimensions","","Profondeur","mm","","950"]
["Façade","Façade-=-Poids-=-kg","","","kg","","5.5"]
["Panneau décoratif 2","Panneau décoratif 2-=-Modèle","","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["Façade 2","Façade 2-=-Dimensions","","Façade 2-=-Dimensions-=-Hauteur-=-mm","mm","","148"]
["","","","Façade 2-=-Dimensions-=-Largeur-=-mm","mm","","950"]
["","","","Façade 2-=-Dimensions-=-Profondeur-=-mm","mm","","950"]
["Raccords de tuyauterie","Gaz","","Type","","","Raccord à dudgeon"]
["","Liquide","","Raccords de tuyauterie-=-Liquide-=-DE-=-mm @","mm","","10"]
["","","","Type","","","Raccord à dudgeon"]
["Raccords de tuyauterie","Gaz","","Piping connections-=-Gas-=-OD-=-mm @","mm","","15.90"]
["Façade 3","Façade 3-=-Dimensions","","Façade 3-=-Dimensions-=-Largeur-=-mm","mm","","950"]
["Panneau décoratif 3","Panneau décoratif 3-=-Modèle","","","","","BYCQ140E2P, BYCQ140E2PB"]
["Façade 3","Façade 3-=-Dimensions","","Façade 3-=-Dimensions-=-Hauteur-=-mm","mm","","106"]
["","","","Façade 3-=-Dimensions-=-Profondeur-=-mm","mm","","950"]
["","Façade 3-=-Poids-=-kg","","","kg","","6.5"]
["Accessoires standard","Washer for hanger bracket","","","","8","8"]
["","Wire clamp material","","","","7","7"]
["","Clamp for drain hose","","","","1","1"]
["","Clamps","","","","1","1"]
["","Drain hose","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Installation guide","","","","1","1"]
["","Insulation for fitting","","","","2","2"]
["","Screws","","","","4","4"]
["","Sealing pads","","","","1","1"]
["Alimentation électrique","Alimentation électrique-=-Tension","","Tension","","","220-240/220"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","","50/60"]
["","Phase","","","","","1~"]
["Courant - 50 Hz","Courant - 50 Hz-=-Intensité maximum de fusible (MFA)-=-A @","","","A","","6"]
["Name","","","","","1","1"]
["Dimensions","Dimensions-=-Unité-=-Largeur","","","mm","840"]
["","Hauteur","","","mm","246"]
["","Dimensions-=-Unité-=-Profondeur","","","mm","840"]
["Unité","kg","","","","24"]
["Puissance frigorifique","Cooling capacity-=-Total capacity-=-At high fan speed","","","kW","11.20"]
["Puissance calorifique","Heating capacity-=-Total capacity-=-At high fan speed","","","kW","12.50"]
["Ventilateur","Débit d'air - 50Hz","","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At high fan speed","m³/min","28.8"]
["","","","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At low fan speed","m³/min","13.8"]
["Puissance absorbée - 50Hz","Power input - 50Hz-=-Cooling-=-At high fan speed","","","kW","0.078"]
["","Power input - 50Hz-=-Heating-=-At high fan speed","","","kW","0.078"]
["Niveau de pression sonore","Sound pressure level-=-Cooling-=-At high fan speed","","","dBA","43.0"]
["","Sound pressure level-=-Cooling-=-At medium fan speed","","","dBA","37.0"]
["","Sound pressure level-=-Heating-=-At high fan speed","","","dBA","43.0"]
["","Sound pressure level-=-Heating-=-At medium fan speed","","","dBA","37.0"]
["","Sound pressure level-=-Cooling-=-At low fan speed","","","dBA","30.0"]
["Sound power level","Sound power level-=-Cooling-=-At high fan speed","","","dBA","60.0"]
["Panneau décoratif","Panneau décoratif-=-Dimensions-=-Largeur","","","mm","950"]
["Niveau de pression sonore","Sound pressure level-=-Heating-=-At low fan speed","","","dBA","30.0"]
["Panneau décoratif","Panneau décoratif-=-Dimensions-=-Hauteur","","","mm","65"]
["Façade 2-=-Poids","kg","","","","10.3"]
["Panneau décoratif","Panneau décoratif-=-Dimensions-=-Profondeur","","","mm","950"]
["Façade-=-Poids","kg","","","","5.5"]
["Façade 2","Façade 2-=-Dimensions-=-Hauteur","","","mm","148"]
["","Façade 2-=-Dimensions-=-Largeur","","","mm","950"]
["","Façade 2-=-Dimensions-=-Profondeur","","","mm","950"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Liquide-=-DE","","","mm","10"]
["Raccords de tuyauterie","Piping connections-=-Gas-=-OD","","","mm","15.90"]
["Façade 3","Façade 3-=-Dimensions-=-Largeur","","","mm","950"]
["","Façade 3-=-Dimensions-=-Hauteur","","","mm","106"]
["","Façade 3-=-Dimensions-=-Profondeur","","","mm","950"]
["Façade 3-=-Poids","kg","","","","6.5"]
["Alimentation électrique","Alimentation électrique-=-Tension","","","","220-240/220"]
["","Alimentation électrique-=-Fréquence","","","","50/60"]
["Courant - 50 Hz-=-Intensité maximum de fusible (MFA)","A","","","","6"]