{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Caisson","Couleur","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","500"]
["","","","Largeur","mm","270"]
["","","","Profondeur","mm","270"]
["Poids","Unité","","","kg","6.8"]
["Mode purification","Puissance absorbée","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Silence","kW","0.008"]
["Niveau de pression sonore","Mode purification","","Turbo","dBA","53"]
["","","","Moyen","dBA","39"]
["","","","Bas","dBA","29"]
["","","","Silence","dBA","19"]
["Ventilateur","Débit d'air","Mode purification","Turbo","m³/h","330"]
["","","","Moyen","m³/h","192"]
["","","","Bas","m³/h","120"]
["","","","Silence","m³/h","66"]
["Dispositifs de sécurité","Élément","","01","","Commutateur de sécurité (le fonctionnement cesse lorsque le capot de l’unité Streamer est ouvert)"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50/60"]
["","Tension","","","Vca","220-240/220-230"]
["Courant de fonctionnement","Mode purification","","Turbo","A","0.32"]
["","","","Moyen","A","0.14"]
["","","","Bas","A","0.10"]
["","","","Silence","A","0.08"]