{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Caisson","Couleur","","","","Blanc"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Hauteur-=-mm","mm","700 (1)"]
["","","","Dimensions-=-Unité-=-Largeur-=-mm","mm","270"]
["","","","Dimensions-=-Unité-=-Profondeur-=-mm","mm","270 (4)"]
["Poids","Unité","","","kg","9.5"]
["Mode purification","Mode purification-=-Puissance absorbée","","Mode purification-=-Puissance absorbée-=-Turbo-=-kW","kW","0.056"]
["","","","Mode purification-=-Puissance absorbée-=-M-=-kW","kW","0.017"]
["","","","Mode purification-=-Puissance absorbée-=-L-=-kW","kW","0.010"]
["","","","Mode purification-=-Puissance absorbée-=-Silence-=-kW","kW","0.007"]
["Mode humidification","Mode humidification-=-Puissance absorbée","","Mode humidification-=-Puissance absorbée-=-Turbo-=-kW","kW","0.058"]
["","","","Mode humidification-=-Puissance absorbée-=-M-=-kW","kW","0.019"]
["","","","Mode humidification-=-Puissance absorbée-=-L-=-kW","kW","0.014"]
["","","","Mode humidification-=-Puissance absorbée-=-Silence-=-kW","kW","0.011"]
["","Mode humidification-=-Capacité du réservoir d'eau-=-L","","","L","2.7"]
["Niveau de pression sonore","Niveau de pression sonore-=-Mode purification","","Niveau de pression sonore-=-Mode purification-=-Turbo-=-dBA","dBA","53.0"]
["","","","Niveau de pression sonore-=-Mode purification-=-Moyen-=-dBA","dBA","39.0"]
["","","","Niveau de pression sonore-=-Mode purification-=-Bas-=-dBA","dBA","29.0"]
["","","","Niveau de pression sonore-=-Mode purification-=-Silence-=-dBA","dBA","19.0"]
["","Niveau de pression sonore-=-Mode humidification","","Niveau de pression sonore-=-Mode humidification-=-Turbo-=-dBA","dBA","53.0"]
["","","","Niveau de pression sonore-=-Mode humidification-=-Moyen-=-dBA","dBA","39.0"]
["","","","Niveau de pression sonore-=-Mode humidification-=-Bas-=-dBA","dBA","33.0"]
["","","","Niveau de pression sonore-=-Mode humidification-=-Silence-=-dBA","dBA","25.0"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Mode purification","Ventilateur-=-Débit d'air-=-Mode purification-=-Turbo-=-m³/h","m³/h","330"]
["","","","Ventilateur-=-Débit d'air-=-Mode purification-=-Moyen-=-m³/h","m³/h","192"]
["","","","Ventilateur-=-Débit d'air-=-Mode purification-=-Bas-=-m³/h","m³/h","120"]
["","","","Ventilateur-=-Débit d'air-=-Mode purification-=-Silence-=-m³/h","m³/h","54"]
["","","Ventilateur-=-Débit d'air-=-Mode humidification","Ventilateur-=-Débit d'air-=-Mode humidification-=-Turbo-=-m³/h","m³/h","330"]
["","","","Ventilateur-=-Débit d'air-=-Mode humidification-=-Moyen-=-m³/h","m³/h","192"]
["","","","Ventilateur-=-Débit d'air-=-Mode humidification-=-Bas-=-m³/h","m³/h","144"]
["","","","Ventilateur-=-Débit d'air-=-Mode humidification-=-Silence-=-m³/h","m³/h","102"]
["Accessoires standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Alimentation électrique","Alimentation électrique-=-Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence-=-Hz","","","Hz","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","Vca","220-240/220-230"]
["Courant de fonctionnement","Courant de fonctionnement-=-Mode purification","","Courant de fonctionnement-=-Mode purification-=-Turbo-=-A","A","0.50"]
["","","","Courant de fonctionnement-=-Mode purification-=-Moyen-=-A","A","0.19"]
["","","","Courant de fonctionnement-=-Mode purification-=-Bas-=-A","A","0.12"]
["","","","Courant de fonctionnement-=-Mode purification-=-Silence-=-A","A","0.09"]
["","Courant de fonctionnement-=-Mode humidification","","Courant de fonctionnement-=-Mode humidification-=-Turbo-=-A","A","0.50"]
["","","","Courant de fonctionnement-=-Mode humidification-=-Moyen-=-A","A","0.20"]
["","","","Courant de fonctionnement-=-Mode humidification-=-Bas-=-A","A","0.15"]
["","","","Courant de fonctionnement-=-Mode humidification-=-Silence-=-A","A","0.13"]
["Remarques","","","","","(1) - Triphase uniquement"]
["","","","","","(2) - Autre fonction : Fonction de redémarrage automatique."]
["","","","","","(3) - Safety valve"]
["","","","","","(4) - Test à Ta BS/BH 14°C/13°C. Conformément à la norme EN 16147."]