{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Mode purification","Ventilateur-=-Débit d'air-=-Mode purification-=-Bas-=-m³/h","m³/h","132"]
["","","Ventilateur-=-Débit d'air-=-Mode humidification","Ventilateur-=-Débit d'air-=-Mode humidification-=-Bas-=-m³/h","m³/h","132"]
["","","","Ventilateur-=-Débit d'air-=-Mode humidification-=-Turbo-=-m³/h","m³/h","420"]
["","","","Ventilateur-=-Débit d'air-=-Mode purification-=-Moyen-=-m³/h","m³/h","210"]
["Mode humidification","Mode humidification-=-Puissance absorbée","","Mode humidification-=-Puissance absorbée-=-L-=-kW","kW","0.012"]
["Mode purification","Mode purification-=-Puissance absorbée","","Mode purification-=-Puissance absorbée-=-Silence-=-kW","kW","0.008"]
["Mode humidification","Mode humidification-=-Capacité du réservoir d'eau-=-L","","","L","3.6"]
["Mode purification","Mode purification-=-Puissance absorbée","","Mode purification-=-Puissance absorbée-=-M-=-kW","kW","0.016"]
["Mode humidification","Mode humidification-=-Puissance absorbée","","Mode humidification-=-Puissance absorbée-=-Silence-=-kW","kW","0.011"]
["","","","Mode humidification-=-Puissance absorbée-=-M-=-kW","kW","0.018"]
["Mode purification","Mode purification-=-Puissance absorbée","","Mode purification-=-Puissance absorbée-=-L-=-kW","kW","0.010"]
["Mode humidification","Mode humidification-=-Puissance absorbée","","Mode humidification-=-Puissance absorbée-=-Turbo-=-kW","kW","0.068"]
["Application","","","","","Type console carrossée"]
["Poids","Unité","","","kg","12.5"]
["Mode purification","Mode purification-=-Puissance absorbée","","Mode purification-=-Puissance absorbée-=-Turbo-=-kW","kW","0.066"]
["Niveau de pression sonore","Niveau de pression sonore-=-Mode humidification","","Niveau de pression sonore-=-Mode humidification-=-Silence-=-dBA","dBA","23"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Mode purification","Ventilateur-=-Débit d'air-=-Mode purification-=-Silence-=-m³/h","m³/h","60"]
["Niveau de pression sonore","Niveau de pression sonore-=-Mode humidification","","Niveau de pression sonore-=-Mode humidification-=-Bas-=-dBA","dBA","27"]
["","","","Niveau de pression sonore-=-Mode humidification-=-Turbo-=-dBA","dBA","54"]
["Surface applicable-=-m²","m²","","","","48, 96"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Mode purification","Ventilateur-=-Débit d'air-=-Mode purification-=-Turbo-=-m³/h","m³/h","420"]
["Niveau de pression sonore","Niveau de pression sonore-=-Mode purification","","Niveau de pression sonore-=-Mode purification-=-Silence-=-dBA","dBA","18"]
["","","","Niveau de pression sonore-=-Mode purification-=-Turbo-=-dBA","dBA","54"]
["","","","Niveau de pression sonore-=-Mode purification-=-Moyen-=-dBA","dBA","37"]
["","Niveau de pression sonore-=-Mode humidification","","Niveau de pression sonore-=-Mode humidification-=-Moyen-=-dBA","dBA","37"]
["","","","Niveau de pression sonore-=-Mode purification-=-Bas-=-dBA","dBA","27"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Mode humidification","Ventilateur-=-Débit d'air-=-Mode humidification-=-Moyen-=-m³/h","m³/h","210"]
["","","","Ventilateur-=-Débit d'air-=-Mode humidification-=-Silence-=-m³/h","m³/h","102"]
["Caisson","Couleur","","","","Blanc (N9. 0)"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Profondeur-=-mm","mm","287"]
["","","","Dimensions-=-Unité-=-Largeur-=-mm","mm","395"]
["Type","","","","","Purificateur-humidificateur de l'air"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Hauteur-=-mm","mm","600"]
["CADR","m³/h","","","","375"]
["Méthode de collecte des poussières","","","","","Filtre HEPA électrostatique"]
["Deodorizing method","","","","","Flash Streamer + catalyseur purificateur"]
["Accessoires standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Alimentation électrique","Alimentation électrique-=-Fréquence","","Alimentation électrique-=-Fréquence-=-Hz","","50/60"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240/220-230"]
["","Alimentation électrique-=-Phase","","","","1~"]
["Cordon d'alimentation","m","","","","2.0"]
["Remarques","","","","","(1) - Converti aux normes NRCC depuis les valeurs de test en conformité avec la norme JEM1467."]
["","","","","","(2) - La zone de couverture est appropriée pour un fonctionnement de l'unité à vitesse max. de ventilation (HH). La zone de couverture fait référence à l'espace dans lequel une certaine quantité de particules de poussière peut être supprimée en 30 minutes."]
["","","","","","(3) - Les niveaux de pression sonore correspondent à la moyenne des valeurs mesurées à 1 m de distance de l'avant, des côtés gauche et droit, et du dessus de l'unité. (Ils sont égaux aux valeurs en chambre anéchoïde)"]