{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B"]
["Dimensions","Unité","","Hauteur","mm","990"]
["","","","Largeur","mm","940"]
["","","","Profondeur","mm","320"]
["Poids","Unité","","","kg","67"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-15"]
["","","","Max.","°CBS","50"]
["","Chauffage","Temp. ext.","Min.","°CBH","-20"]
["","","","Max.","°CBH","15.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","64"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48"]
["","Chauffage","","Nom.","dBA","50"]
["","Mode Nuit","","Niveau 1","dBA","43"]
["Réfrigérant","Type","","","","R-32"]
["","Charge","","","kg","2.6"]
["Réfrigérant","PRP","","","","675"]
["Réfrigérant","Charge","","","tCO2Eq","1.8"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52"]
["Raccords de tuyauterie","Gaz","","DE","mm","15.9"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","55"]
["","","Système","Équivalente","m","75"]
["","","","Préchargé d'usine jusqu'à","m","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","Voir le manuel d'installation"]
["","Dénivelé","UI - UE","Max.","m","30.0"]
["","","UI - UI","Max.","m","0.5"]
["Accessoires standard","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Alimentation électrique","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50/60"]
["","Alimentation électrique-=-Tension","","Tension","","220-240"]