{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A"]
[]
[]
[]
[]
["","","","","","2MXM40A2V1B","2MXM50A2V1B","2MXM68A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","","552","734"]
["","","","Breedte","mm","","852","974"]
["","","","Diepte","mm","","350","408"]
["Gewicht","Unit","","","kg","","41","60"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","Omgeving","Min.","°C DB","","-10","-10"]
["","","","Max.","°C DB","","46","46"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","","48","48"]
["","Verwarmen","","Nom.","dBA","","50","48"]
["Koelmiddel","Type","","","","","R-32","R-32"]
["","Vulling","","","kg","","1.15","2.00"]
["","GWP","","","","","675","675"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Hoogteverschil","IU - OU","Max.","m","","15","15"]
["","","IU - IU","Max.","m","","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","30","50"]
["Standaard-accessoires","Montagehandleiding","","","","","1","1"]
["","Zakje schroeven","","","","","1","1"]
["","Aftapplug","","","","","1","1"]
["","Montage verloopstuk","","","","","1","1"]
["Power supply","Fase","","","","","1~","1~"]
["","Frequentie","","","Hz","","50","50"]
["","Spanning","","","V","","220-240","220-240"]
["Opmerkingen","","","","","(1) - Van één kamer","(1) - Van één kamer","(1) - Van één kamer"]
["","","","","","(2) - Voor een combinatie met CVXM-A, FVXM-A - de maximale leidinglengte is 30m.","(2) - Voor een combinatie met CVXM-A, FVXM-A - de maximale leidinglengte is 30m.","(2) - Voor een combinatie met CVXM-A, FVXM-A - de maximale leidinglengte is 30m."]
["","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","(4) - Voor elektrische gegevens zie afzonderlijke tekening","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(5) - Bevat gefluoreerde broeikasgassen","(5) - Bevat gefluoreerde broeikasgassen","(5) - Bevat gefluoreerde broeikasgassen"]
["Afmetingen","Unit","","Hoogte","mm","552"]
["","","","Breedte","mm","852"]
["","","","Diepte","mm","350"]
["Gewicht","Unit","","","kg","36"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Werkingsbereik-=-Koelen","Werkingsbereik-=-Koelen-=- ","Werkingsbereik-=-Koelen-=- -=-Min.-=-°CDB","°C DB","-10"]
["","","","Werkingsbereik-=-Koelen-=- -=-Max.-=-°CDB","°C DB","46"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dBA","46"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dBA","48"]
["Koelmiddel","Type","","","","R-32"]
["Koudemiddel","Koudemiddel-=-Inhoud-=-kg","","","kg","0.88"]
["","Vulling","","","tCO2Eq","0.60"]
["Koelmiddel","GWP","","","","675"]
["Koelleidingmaten","Koelleidingmaten-=-Leidinglengte","Koelleidingmaten-=-Leidinglengte-=- ","Koelleidingmaten-=-Leidinglengte-=- -=-Max.-=-m","m","20 (1)"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)"]
["Koelleidingmaten","Koelleidingmaten-=-Hoogteverschil","Koelleidingmaten-=-Hoogteverschil-=- ","Koelleidingmaten-=-Hoogteverschil-=- -=-Max.-=-m","m","15"]
["","","Koelleidingmaten-=-Hoogteverschil-=-IU - IU","Koelleidingmaten-=-Hoogteverschil-=-IU - IU-=-Max.-=-m","m","7.5"]
["","Koelleidingmaten-=-Totale leidinglengte","Koelleidingmaten-=-Totale leidinglengte-=-Systeem","Koelleidingmaten-=-Totale leidinglengte-=-Systeem-=-Werkelijk-=-m","m","30"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240"]
["Standaard-accessoires","Afvoerdop","","","","","","3"]