{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA50A2VEB","ADEA100A2VEB"]
["Ventilator","Externe statische druk","","Hoog","Pa","","150"]
["Behuizing","Kleur","","","","","Niet gelakt (gegalvaniseerd)"]
["Behuizing","Materiaal","","","","","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","","245"]
["","","","Breedte","mm","","1400"]
["","","","Diepte","mm","","800"]
["Gewicht","Unit","","","kg","","46"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","","29"]
["Ventilator","Luchtdebiet","Koelen","Middelhoog","m³/min","","26"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","","23"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","","29"]
["Ventilator","Luchtdebiet","Verwarmen","Middelhoog","m³/min","","26"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","","23"]
["Ventilator","Externe statische druk","","Nom.","Pa","","40"]
["Geluidsvermogenniveau","Koelen","","","dBA","","58"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","","34"]
["Geluidsdrukniveau","Koelen","","Middelhoog","dBA","","32"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","","30"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","","36"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dBA","","33"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","","30"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","9.52"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","","15.9"]
["Leidingaansluitingen","Drainage","","","","","VP20 (I.D. 20/O.D. 26)"]
["Afvoerhoogte","mm","","","","","625"]
["Besturingssystemen","Infrared remote control","","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Installation manual","","","","","1"]
["","Washer for hanger bracket","","","","","8"]
["","Operation manual","","","","","1"]
["","Clamps","","","","","4"]
["","Drain hose","","","","","1"]
["","Insulation for fitting","","","","","2"]
["","Metal clamp for drain hose","","","","","1"]
["","Screws","","","","","40"]
["","Sealing pads","","","","","5"]
["Voeding","Fase","","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","","50"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","","220-240/220"]
["Standaard-accessoires","AAA dry-cell batteries","","","","3"]