{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M"]
[]
[]
[]
[]
["","","","","","CTXM15M2V1B"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dBA","34"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Nom.-=-m³/min","m³/min","8.7"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dBA","33"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Nom.-=-m³/min","m³/min","7.9"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","294"]
["","","","Breedte","mm","811"]
["","","","Diepte","mm","272"]
["Gewicht","Unit","","","kg","10"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","11.1"]
["","","","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","6.0"]
["","","","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Fluisterstille werking-=-m³/min","m³/min","4.4"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","10.4"]
["","","","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","6.5"]
["","","","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Fluisterstille werking-=-m³/min","m³/min","5.3"]
["Geluidsvermogenniveau","Koelen","","","dBA","57"]
["","Verwarmen","","","dBA","54"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","41"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","25"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dBA","19"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","39"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","26"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dBA","20"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","9.5"]
["Leidingaansluitingen","Drainage","","","","18"]
["Besturingssystemen","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","1"]
["Voeding","Naam","","","","V1"]
["","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie-=-Hz","","","Hz","50"]
["","Spanningsvorm-=-Spanning-=-V","","","V AC","220-240"]