{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","Test TC160075","EGSQH10S18AA9W"]
["Opmerkingen","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)","(1) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)","(2) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(3) - met 40% propyleenglycol","(3) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m van de unit. Het is een relatieve waarde die afhangt van de afstand en de akoestische omgeving."]
["","","","","","(4) - Warmteverlies volgens EN12897","(4) - Inclusief leidingen + PHE + back-upverwarming; exclusief expansievat"]
["","","","","","(5) - Inclusief leidingen + PHE + back-upverwarming; exclusief expansievat","(5) - Warmteverlies volgens EN12897"]
["","","","","","(6) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m van de unit. Het is een relatieve waarde die afhangt van de afstand en de akoestische omgeving.","(6) - Met warmtepomp + back-upverwarming"]
["","","","","","(7) - Met warmtepomp","(7) - Met warmtepomp"]
["","","","","","(8) - Met warmtepomp + back-upverwarming","(8) - Met back-upverwarming"]
["","","","","","(9) - Met back-upverwarming","(9) - met 40% propyleenglycol"]
["Totale verwarmingscapaciteit","Totale verwarmingscapaciteit-=-Min.-=-kW","","","kW","","3.11, 2.47"]
["","Totale verwarmingscapaciteit-=-Nom.-=-kW","","","kW","","10.3, 9.2"]
["","Totale verwarmingscapaciteit-=-Max.-=-kW","","","kW","","13, 11.9"]
["Opgenomen vermogen","Opgenomen vermogen-=-Nom.-=-kW","","","kW","","2.38, 2.89"]
["COP","","","","","","4.33, 3.18"]
["Behuizing","Kleur","","","","","Wit"]
["Behuizing","Behuizing-=-Materiaal","","","","","Voorgelakte metaalplaat"]
["Afmetingen","Afmetingen-=-Unit","","Afmetingen-=-Unit-=-Hoogte-=-mm","mm","","1730"]
["","","","Afmetingen-=-Unit-=-Breedte-=-mm","mm","","600"]
["","","","Afmetingen-=-Unit-=-Diepte-=-mm","mm","","728"]
["Gewicht","Unit","","","kg","","210"]
["Tank","Tank-=-Watervolume-=-l","","","l","","180"]
["","Tank-=-Isolatie","","Tank-=-Isolatie-=-Warmteverlies-=-kWh/24h","kWu/24u","","1.36"]
["","Tank-=-Corrosiebescherming","","","","","Anode"]
["Koelmiddel","Koelmiddel-=-Type","","","","","R-410A"]
["Koelmiddel","GWP","","","","","2090"]
["Koudemiddel","Koudemiddel-=-Vulling-=-tCO2eq","","","tCO2Eq","","3.76"]
["","Koudemiddel-=-Inhoud-=-kg","","","kg","","1.8"]
["Verwarming","Verwarming-=-Wateruitlaat gematigd klimaat 55°C","Verwarming-=-Wateruitlaat gematigd klimaat 55°C-=-Algemeen","Verwarming-=-Wateruitlaat gematigd klimaat 55°C-=-Algemeen-=-SCOP","","","3.68"]
["","","","Verwarming-=-Wateruitlaat gematigd klimaat 55°C-=-Algemeen-=-Seizoensefficiëntieklasse verwarming","","","A++"]
["","Verwarming-=-Wateruitlaat gematigd klimaat 35°C","Verwarming-=-Wateruitlaat gematigd klimaat 35°C-=-Algemeen","Verwarming-=-Wateruitlaat gematigd klimaat 35°C-=-Algemeen-=-SCOP","","","5.06"]
["","","","Verwarming-=-Wateruitlaat gematigd klimaat 35°C-=-Algemeen-=-Seizoensefficiëntieklasse verwarming","","","A+++"]
["Voeding","Voeding-=-Naam","","","","","9W"]
["","Voeding-=-Fase","","","","","3~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","","50"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","","400"]
["Stroom","Current-=-Recommended fuses","","Aanbevolen zekeringen","","","25"]