{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","","FCAHG71FVEB"]
["Behuizing","Materiaal","","","","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","288"]
["","","","Breedte","mm","840"]
["","","","Diepte","mm","840"]
["Gewicht","Unit","","","kg","25.0"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","21.2"]
["Ventilator","Luchtdebiet","Koelen","Middelhoog","m³/min","16.7"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","12.2"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","21.2"]
["Ventilator","Luchtdebiet","Verwarmen","Middelhoog","m³/min","16.7"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","12.2"]
["Geluidsvermogenniveau","Koelen","","","dBA","53"]
["","Verwarmen","","","dBA","53"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","36"]
["Geluidsdrukniveau","Koelen","","Middelhoog","dBA","33"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","29"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","36"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dBA","33"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","29"]
["Koelmiddel","GWP","","","","675"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","15.9"]
["Leidingaansluitingen","Drainage","","","","VP25 (I.D. 25/O.D. 32)"]
["Sierpaneel","Model","","","","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas"]
["","Kleur","","","","Zuiver wit (RAL 9010)"]
["","Afmetingen","","Hoogte","mm","130"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","950"]
["Uitblaaspaneel","Uitblaaspaneel-=-Gewicht-=-kg","","","kg","10"]
["Sierpaneel 2","Model","","","","BYCQ140DG: zelfreinigend paneel"]
["Uitblaaspaneel 2","Uitblaaspaneel 2-=-Kleur","","","","Zuiver wit (RAL 9010)"]
["","Uitblaaspaneel 2-=-Afmetingen","","Uitblaaspaneel 2-=-Afmetingen-=-H-=-mm","mm","130"]
["","","","Uitblaaspaneel 2-=-Afmetingen-=-B-=-mm","mm","950"]
["","","","Uitblaaspaneel 2-=-Afmetingen-=-D-=-mm","mm","950"]
["","Uitblaaspaneel 2-=-Gewicht-=-kg","","","kg","10.3"]
["Sierpaneel 3","Model","","","","BYCQ140DW: volledig wit, Zie opmerking 1"]
["Uitblaaspaneel 3","Uitblaaspaneel 3-=-Kleur","","","","Zuiver wit (RAL 9010)"]
["","Uitblaaspaneel 3-=-Afmetingen","","Uitblaaspaneel 3-=-Afmetingen-=-H-=-mm","mm","50"]
["","","","Uitblaaspaneel 3-=-Afmetingen-=-B-=-mm","mm","950"]
["","","","Uitblaaspaneel 3-=-Afmetingen-=-D-=-mm","mm","950"]
["","Uitblaaspaneel 3-=-Gewicht-=-kg","","","kg","5.4"]
["Decoratiepaneel 4","Decoratiepaneel 4-=-Model","","","","BYCQ140D: wit met grijze lamellen"]
["","Decoratiepaneel 4-=-Kleur","","","","Zuiver wit (RAL 9010)"]
["","Decoratiepaneel 4-=-Afmetingen","","Decoratiepaneel 4-=-Afmetingen-=-Hoogte-=-mm","mm","50"]
["","","","Decoratiepaneel 4-=-Afmetingen-=-Breedte-=-mm","mm","950"]
["","","","Decoratiepaneel 4-=-Afmetingen-=-Diepte-=-mm","mm","950"]
["","Decoratiepaneel 4-=-Gewicht-=-kg","","","kg","5.4"]
["Standaard-accessoires","Installation manual","","","","Installation manual"]
["","Installation and operation manual","","","","Installation and operation manual"]
["Voeding","Naam","","","","VE"]
["","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50/60"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240"]