{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":9,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB"]
[]
[]
[]
[]
["","","","","","FTXJ25A2V1BB (Archived)","FTXJ35A2V1BB (Archived)","FTXJ42A2V1BB (Archived)","FTXJ50A2V1BB (Archived)"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","40","41","45","46"]
["","","","Middelhoog","dBA","33","33","37","42"]
["","","","Fluisterstille werking","dBA","19","19","21","24"]
["","","","Laag","dBA","25","25","29","33"]
["","Koelen","","Middelhoog","dBA","33","33","37","39"]
["","","","Fluisterstille werking","dBA","19","19","21","24"]
["","","","Laag","dBA","25","25","29","31"]
["","","","Hoog","dBA","40","41","45","46"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1","1"]
["","Draadloze afstandsbediening","","","","1","1","1","1"]
["","Afstandsbedieningshouder","","","","1","1","1","1"]
["","AAA drogecelbatterij","","","","2","2","2","2"]
["","Geurfilter van titaniumapatiet","","","","1","1","1","1"]
["","Zilverpartikelfilter","","","","1","1","1","1"]
["","Schroefdeksel","","","","2","2","2","2"]
["","Zakje schroeven","","","","1","1","1","1"]
["","Algemene voorzorgsmaatregelen","","","","1","1","1","1"]
["","Montageplaat","","","","1","1","1","1"]
["Koelmiddel","GWP","","","","675","675","675","675"]
["Besturingssystemen","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC488A1K","ARC488A1K","ARC488A1K","ARC488A1K"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","12.7","12.7"]
["","Afvoer","","","","18","18","18","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.022","0.024","0.028","0.031"]
["","Verwarmen","","Nom.","kW","0.022","0.024","0.036","0.039"]
["Sound power level","Koelen","","","dBA","57","60","60","60"]
["Afmetingen","Unit","","Breedte","mm","900","900","900","900"]
["","","","Diepte","mm","212","212","212","212"]
["","","","Hoogte","mm","305","305","305","305"]
["Behuizing","Kleur","","","","Zwart","Zwart","Zwart","Zwart"]
["Gewicht","Unit","","","kg","12","12","12","12"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","11.3","11.7","14.4","15.0"]
["","","","Middelhoog","m³/min","9.0","9.0","10.5","11.1"]
["","","","Laag","m³/min","6.4","6.4","7.7","8.2"]
["","","","Fluisterstille werking","m³/min","4.6","4.6","5.2","5.7"]
["","","Koelen","Laag","m³/min","6.0","6.0","7.2","7.6"]
["","","","Middelhoog","m³/min","8.6","8.6","9.5","10.4"]
["","","","Hoog","m³/min","11.4","11.8","13.0","13.5"]
["","","","Fluisterstille werking","m³/min","4.6","4.6","4.6","5.2"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Naam","","","","V1","V1","V1","V1"]
["","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]