{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ50MV1BS"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","47"]
["","","","Middelhoog","dBA","","41"]
["","","","Fluisterstille werking","dBA","","25"]
["","","","Laag","dBA","","35"]
["","Koelen","","Middelhoog","dBA","","40"]
["","","","Fluisterstille werking","dBA","","25"]
["","","","Laag","dBA","","35"]
["","","","Hoog","dBA","","46"]
["Standaard-accessoires","Bedieningshandleiding","","","","","1"]
["","Montagehandleiding","","","","","1"]
["","Draadloze afstandsbediening","","","","","1"]
["","AAA drogecelbatterij","","","","","2"]
["","Afstandsbedieningshouder","","","","","1"]
["","Montageschroeven voor montageplaat","","","","","5"]
["","Montageplaat","","","","","1"]
["","Geurfilter van titaniumapatiet","","","","","2"]
["","Borgschroef voor houder van afstandsbediening","","","","","2"]
["","Montageschroeven binnenunit","","","","","2"]
["","Schroefdeksel","","","","","2"]
["","W-LAN-adapterkit","","","","","1"]
["Besturingssystemen","Infrared remote control","","","","","ARC466A9"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","6.35"]
["","Gas","","Buitendiameter","mm","","12.70"]
["","Afvoer","","","","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","0.033"]
["","Verwarmen","","Nom.","kW","","0.043"]
["Sound power level","Koelen","","","dBA","","60"]
["","Verwarmen","","","dBA","","60"]
["Afmetingen","Unit","","Breedte","mm","","998"]
["","","","Diepte","mm","","212"]
["","","","Hoogte","mm","","303"]
["Behuizing","Kleur","","","","","Zilver"]
["Gewicht","Unit","","","kg","","12"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","","12.6"]
["","","","Middelhoog","m³/min","","10.5"]
["","","","Laag","m³/min","","8.1"]
["","","","Fluisterstille werking","m³/min","","5.0"]
["","","Koelen","Laag","m³/min","","6.8"]
["","","","Middelhoog","m³/min","","8.9"]
["","","","Hoog","m³/min","","10.9"]
["","","","Fluisterstille werking","m³/min","","3.6"]
["Power supply","Fase","","","","","1~"]
["","Naam","","","","","V1"]
["","Frequentie","","","Hz","","50"]
["","Spanning","","","V","","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.023"]
["","Verwarmen","","Nom.","kW","0.031"]
["Behuizing","Kleur","","","","Zilver"]
["Afmetingen","Unit","","Hoogte","mm","303"]
["","","","Breedte","mm","998"]
["","","","Diepte","mm","212"]
["Gewicht","Unit","","","kg","12"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","8.9"]
["","","Koeling","Middelhoog","m³/min","6.6"]
["","","","Laag","m³/min","4.4"]
["","","","Fluisterstille werking","m³/min","2.6"]
["","","Verwarmen","Hoog","m³/min","10.2"]
["","","Verwarming","Middelhoog","m³/min","8.4"]
["","","Verwarmen","Laag","m³/min","6.3"]
["","","","Fluisterstille werking","m³/min","3.8"]
["Geluidsvermogenniveau","Koelen","","","dBA","54"]
["","Verwarmen","","","dBA","56"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","38"]
["","Koeling","","Middelhoog","dBA","32"]
["","","","Laag","dBA","25"]
["","","","Fluisterstille werking","dBA","19"]
["","Verwarmen","","Hoog","dBA","40"]
["","Verwarming","","Middelhoog","dBA","34"]
["","Verwarmen","","Laag","dBA","28"]
["","","","Fluisterstille werking","dBA","19"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.50"]
["","Drainage","","","","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A9"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","Fixing screw for remote controller holder","","","","2"]
["","WLAN adapter kit","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Fixing screws for mounting plate","","","","5"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Voeding","Naam","","","","V1"]
["","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]