{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":16,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R"]
[]
[]
[]
[]
["","","","","","FTXM20R5V1B","FTXM20R2V1B","FTXM25R2V1B","FTXM25R5V1B","FTXM35R5V1B","FTXM35R2V1B","FTXM42R5V1B","FTXM42R2V1B","FTXM50R2V1B","FTXM60R2V1B","FTXM71R2V1B"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.023","0.023","0.022","0.022","0.027","0.027","0.038","0.038","0.032","0.035","0.06"]
["","Koelen","","Opgenomen vermogen-=-Koelen-=-Nom.-=-kW (2)","kW","0.029","0.029","0.025","0.025","0.030","0.030","0.034","0.034","","0.032"]
["Geluidsvermogenniveau","Verwarmen","","","dBA","54","54","54","54","54","54","60","60","58","59","61"]
["Besturingssystemen","Infrared remote control","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","10.5","10.5","10.5","10.5","11.3","11.3","11.9","11.9","","16.7"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","9.3","9.3","9.8","9.8","9.8","9.8","12.4","12.4","","16.5"]
["","","","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","5.7","5.7","5.7","5.7","6.0","6.0","6.5","6.5","","11.8"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","6.2","6.2","6.3","6.3","6.5","6.5","6.5","6.5","","12.4"]
["Afmetingen","Unit","","Breedte","mm","778","778","778","778","778","778","778","778","998","998","998"]
["","","","Hoogte","mm","295","295","295","295","295","295","295","295","299","299","299"]
["","","","Diepte","mm","272","272","272","272","272","272","272","272","292","292","292"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dBA","20","20","20","20","20","20","21","21","","33"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Fluisterstille werking-=-m³/min","m³/min","5.1","5.1","4.9","4.9","4.9","4.9","4.9","4.9","","11.1"]
["","","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Fluisterstille werking-=-m³/min","m³/min","4.3","4.3","4.1","4.1","4.2","4.2","4.3","4.3","","9.1"]
["Geluidsdrukniveau","Koelen","","Middelhoog","dBA","33","33","33","33","33","33","39","39","","42"]
["Ventilator","Luchtdebiet","Verwarmen","Middelhoog","m³/min","8.2","8.2","8","8","8.5","8.5","9.7","9.7","","15.2"]
["","","Koelen","Middelhoog","m³/min","7.5","7.5","7.6","7.6","7.8","7.8","9.0","9.0","","14.0"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dBA","34","34","34","34","35","35","39","39","39","41","42"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","41","41","41","41","45","45","45","45","","46"]
["Gewicht","Unit","","","kg","10","10.0","10","10","10.0","10.0","10.0","10.0","","14.5"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","25","25","25","25","29","29","30","30","","37"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","9.5","9.50","9.5","9.5","9.50","9.50","9.50","9.50","","12.7"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dBA","19","19","19","19","19","19","21","21","","30"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit","Wit","Wit","Wit","Wit","","Wit"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","26","26","27","27","28","28","29","29","","36"]
["Geluidsvermogenniveau","Koelen","","","dBA","57","57","57","57","58","58","60","60","58","60","60"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","39","39","39","39","39","39","45","45","","45"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","","","","","","","","0.03","","0.054"]
["Leidingaansluitingen","Drainage","","","","18","18","18","18","18","18","18","18","18","18","18"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","1","1","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1","1","1"]
["Voeding","Naam","","","","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","","220-240"]
["","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50","50","50","50","50","50","50","50","","50"]
["Behuizing","Kleur","","","","","","","","","","","","Wit","","Wit"]
["Gewicht","Unit","","","kg","","","","","","","","","14.5","","14.5"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","","","","","","","","15.8","","16.9"]
["","","Koeling","Middelhoog","m³/min","","","","","","","","","14","","15"]
["","","","Laag","m³/min","","","","","","","","","11.4","","12.2"]
["","","","Fluisterstille werking","m³/min","","","","","","","","","8.3","","10"]
["","","Verwarmen","Hoog","m³/min","","","","","","","","","15.8","","17.7"]
["","","Verwarming","Middelhoog","m³/min","","","","","","","","","14.2","","15.8"]
["","","Verwarmen","Laag","m³/min","","","","","","","","","12","","12.7"]
["","","","Fluisterstille werking","m³/min","","","","","","","","","10.5","","11.6"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","","","","","","","","44","","47"]
["","Koeling","","Middelhoog","dBA","","","","","","","","","40","","43"]
["","","","Laag","dBA","","","","","","","","","36","","38"]
["","","","Fluisterstille werking","dBA","","","","","","","","","27","","32"]
["","Verwarmen","","Hoog","dBA","","","","","","","","","43","","46"]
["","","","Laag","dBA","","","","","","","","","34","","37"]
["","","","Fluisterstille werking","dBA","","","","","","","","","31","","34"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","","","","","","","","","12.7","","15.9"]
["Regelsystemen","Bedrade afstandsbediening","","","","","","","","","","","","BRC073A1","","BRC073A1"]
["Standaard-accessoires","Silver particle filter","","","","","","","","","","","","1","1","1"]
["Spanningsvoeding","Spanningsvoeding-=-Frequentie","","Frequentie","","","","","","","","","","50","","50"]
["","Spanningsvoeding-=-Spanning","","Spanning","","","","","","","","","","220-240","","220-240"]