{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M"]
[]
[]
[]
[]
["","","","","","FTXP25M5V1B","FTXP35M5V1B","FTXP50M2V1B","FTXP60M2V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","40","40","38","40"]
["","","","Middelhoog","dBA","34","35","33","35"]
["","","","Fluisterstille werking","dBA","21","21"]
["","","","Laag","dBA","28","29","30","32"]
["","Koelen","","Middelhoog","dBA","33","34","39","41"]
["","","","Fluisterstille werking","dBA","19","20","27","30"]
["","","","Laag","dBA","26","27","34","36"]
["","","","Hoog","dBA","40","43","43","45"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1","1"]
["","Infrarood-afstandsbediening","","","","1","1","1","1"]
["","AAA drogecelbatterij","","","","2","2","2","2"]
["","Afstandsbedieningshouder","","","","1","1","1","1"]
["","Montageplaat","","","","1","1","1","1"]
["","Geurfilter van titaniumapatiet","","","","2","2","1","1"]
["","Montageschroeven binnenunit","","","","2","2","2","2"]
["Besturingssystemen","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53","ARC480A53"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","12.7","12.7"]
["","Afvoer","","","","18","18","18","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.020","0.032","0.029","0.032"]
["","Verwarmen","","Nom.","kW","0.023","0.032","0.032","0.035"]
["Sound power level","Koelen","","","dBA","55","58","59","60"]
["","Verwarmen","","","dBA","55","58","61","62"]
["Afmetingen","Unit","","Breedte","mm","770","770","990","990"]
["","","","Diepte","mm","225","225","263","263"]
["","","","Hoogte","mm","286","286","295","295"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit"]
["Gewicht","Unit","","","kg","8.50","9.00","13.5","13.5"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","10.4","11.5","17.3","17.9"]
["","","","Middelhoog","m³/min","8.1","9.0","14.4","15.3"]
["","","","Laag","m³/min","6.4","7.0","11.8","12.4"]
["","","","Fluisterstille werking","m³/min","5.2","5.3","10.4","11.0"]
["","","Koelen","Laag","m³/min","5.8","6.3","11.5","11.8"]
["","","","Middelhoog","m³/min","7.7","8.3","14.0","14.4"]
["","","","Hoog","m³/min","9.7","11.5","16.3","16.8"]
["","","","Fluisterstille werking","m³/min","4.2","4.5","8.3","9.2"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Naam","","","","","","V1","V1"]
["","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]
["Standaard-accessoires","Zilverpartikelfilter","","","","","","1","1"]