{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP35M5V1B9"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","40"]
["","","","Middelhoog","dBA","35"]
["","","","Fluisterstille werking","dBA","21"]
["","","","Laag","dBA","29"]
["","Koelen","","Middelhoog","dBA","34"]
["","","","Fluisterstille werking","dBA","20"]
["","","","Laag","dBA","27"]
["","","","Hoog","dBA","43"]
["Besturingssystemen","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A53"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.50"]
["","Afvoer","","","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.032"]
["","Verwarmen","","Nom.","kW","0.032"]
["Sound power level","Koelen","","","dBA","58"]
["","Verwarmen","","","dBA","58"]
["Afmetingen","Unit","","Breedte","mm","770"]
["","","","Diepte","mm","225"]
["","","","Hoogte","mm","286"]
["Behuizing","Kleur","","","","Wit"]
["Gewicht","Unit","","","kg","9.00"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","11.5"]
["","","","Middelhoog","m³/min","9.0"]
["","","","Laag","m³/min","7.0"]
["","","","Fluisterstille werking","m³/min","5.3"]
["","","Koelen","Laag","m³/min","6.3"]
["","","","Middelhoog","m³/min","8.3"]
["","","","Hoog","m³/min","11.5"]
["","","","Fluisterstille werking","m³/min","4.5"]
["Power supply","Fase","","","","1~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]