{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.03","0.030","0.030"]
["","Koelen","","Opgenomen vermogen-=-Koelen-=-Nom.-=-kW (2)","kW","0.03","0.030","0.030"]
["Geluidsvermogenniveau","Verwarmen","","","dBA","56","57","59"]
["Besturingssystemen","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","10.7","12.1","15.0"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","11.7","13.3","14.4"]
["","","","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","5.3","5.6","6.6"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","6.7","6.9","7.7"]
["Afmetingen","Unit","","Breedte","mm","798","798","798"]
["","","","Hoogte","mm","295","295","295"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Nom.-=-m³/min","m³/min","7.5","8.4","9.2"]
["Afmetingen","Unit","","Diepte","mm","372","372","372"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dBA","19","19","24"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Fluisterstille werking-=-m³/min","m³/min","4.8","4.8","5.9"]
["","","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Fluisterstille werking-=-m³/min","m³/min","4","4.0","4.6"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","38","42","47"]
["Gewicht","Unit","","","kg","15","15","15"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","26","27","30"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","9.5","9.5","9.5"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dBA","19","19","23"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","28","29","31"]
["Geluidsvermogenniveau","Koelen","","","dBA","54","57","60"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","39","42","44"]
["","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dBA","33","35","38"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Nom.-=-m³/min","m³/min","8.6","9.2","10.7"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dBA","35","36","38"]
["Standaard-accessoires","Wireless remote control","","","","1","1","1"]
["","Photocatalytic air purifying and deodorising filter","","","","1","1","1"]
["","Dry batteries","","","","2","2","2"]
["","Indoor unit fixing screws","","","","3","3","3"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Voeding","Naam","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240","220-240","220-240"]
["","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50","50","50"]
["Opmerkingen","","","","","(1) - 230V","(1) - Achterkant van warmtewisselaar","(1) - Achterkant van warmtewisselaar"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - Voorkant van warmtewisselaar","(3) - 230V"]
["","","","","","(4) - Achterkant van warmtewisselaar","(4) - 230V","(4) - Voorkant van warmtewisselaar"]
["","","","","","(5) - Voorkant van warmtewisselaar","(5) - 240V","(5) - 240V"]