{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":12,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAA-A"]
[]
[]
[]
[]
["","","","","","FXAA50AUV1B","FXAA20AUV1B","FXAA40AUV1B","FXAA25AUV1B","FXAA32AUV1B","FXAA63AUV1B","FXAA15AUV1B (Archived)"]
["Leidingaansluitingen","Vloeistof","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","12.70","9.52","12.70","9.52","9.52","12.70","9.52"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6","6","6","6","6","6","6"]
["","Gas","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding"]
["Opgenomen vermogen - 50Hz","Koelen","","Bij hoge ventilatorsnelheid","kW","0.033","0.019","0.025","0.028","0.030","0.050","0.017"]
["Geluidsdrukniveau","Verwarmen","","Bij lage ventilatorsnelheid","dBA","35.5","28.5","33.5","28.5","28.5","38.5","28.5"]
["Leidingaansluitingen","Drainage","","","","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)"]
["Luchtfilter","Type","","","","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar","Verwijderbaar/wasbaar"]
["Ventilator","Luchtdebiet - 50Hz","Koelen","Bij lage ventilatorsnelheid","m³/min","10.9","6.5","9.8","6.5","6.5","12.9","6.5"]
["","","","Bij hoge ventilatorsnelheid","m³/min","14.2","7.9","12.2","8.3","9.4","18.2","7.1"]
["Opgenomen vermogen - 50Hz","Verwarmen","","Bij hoge ventilatorsnelheid","kW","0.039","0.029","0.030","0.034","0.035","0.060","0.025"]
["Geluidsdrukniveau","Koelen","","Bij lage ventilatorsnelheid","dBA","35.5","28.5","33.5","28.5","28.5","38.5","28.5"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","dBA","42.0","34.0","38.0","36.0","38.5","47.0","33.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","39.0","31.5","36.0","32.5","33.5","43.0","31.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","38.5","31.0","35.5","32.0","33.0","42.5","30.5"]
["","","","Bij hoge ventilatorsnelheid","dBA","41.0","33.0","37.0","35.0","37.5","46.5","32.0"]
["Sound power level","Koelen","","Bij hoge ventilatorsnelheid","dBA","58.0","52.0","55.0","53.0","55.0","63.0","51.0"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit","Wit","Wit","Wit"]
["Gewicht","Unit","","","kg","15","12","15","12","12","15","12"]
["Afmetingen","Unit","","Diepte","mm","269","266","269","266","266","269","266"]
["","","","Breedte","mm","1050","795","1050","795","795","1050","795"]
["","","","Hoogte","mm","290","290","290","290","290","290","290"]
["Verwarmingscapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","6.3","2.5","5.0","3.2","4.0","8.0","1.9"]
["Koelcapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","5.6","2.2","4.5","2.8","3.6","7.1","1.7"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Standaard-accessoires","Installation plate","","","","1","1","1","1","1","1","Installation plate"]
["","General safety precautions","","","","1","1","1","1","1","1","General safety precautions"]
["","Wire clamp material","","","","4","4","4","4","4","4","Wire clamp material"]
["","Heat insulating tape","","","","1","1","1","1","1","1","Heat insulating tape"]
["","Installation and operation manual","","","","1","1","1","1","1","1","Installation and operation manual"]
["","Installation pattern","","","","1","1","1","1","1","1","Installation pattern"]
["","Screw bag","","","","1","1","1","1","1","1","Screw bag"]
["Stroom - 50Hz","Stroom - 50Hz-=-Afzekerwaarde-=-A","","","A","6","6","6","6","6","6","6"]
["Voeding","Naam","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50","50","50","50","50","50","50"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]