{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","FXFA125A2VEB","FXFA100A2VEB (Archived)"]
["Standaard-accessoires","Washer for hanger bracket","","","8","Washer for hanger bracket"]
["","Clamp for drain hose","","","1","Clamp for drain hose"]
["","Drain hose","","","1","Drain hose"]
["","Installation and operation manual","","","1","Installation and operation manual"]
["","Installation guide","","","1","Installation guide"]
["","Screws","","","4","Screws"]
["Name","","","","1","7"]
["Afmetingen","Afmetingen-=-Unit-=-Breedte","","mm","840"]
["","Hoogte","","mm","288"]
["","Afmetingen-=-Unit-=-Diepte","","mm","840"]
["Unit","kg","","","26"]
["Koelcapaciteit","Cooling capacity-=-Total capacity-=-At high fan speed","","kW","14.00"]
["Verwarmingscapaciteit","Heating capacity-=-Total capacity-=-At high fan speed","","kW","16.00"]
["Ventilator","Luchtdebiet - 50Hz","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At high fan speed","m³/min","33.0"]
["","","Fan-=-Air flow rate - 50Hz-=-Cooling-=-At low fan speed","m³/min","20.6"]
["Opgenomen vermogen - 50Hz","Power input - 50Hz-=-Cooling-=-At high fan speed","","kW","0.103"]
["","Power input - 50Hz-=-Heating-=-At high fan speed","","kW","0.103"]
["Geluidsdrukniveau","Sound pressure level-=-Cooling-=-At high fan speed","","dBA","45.0"]
["","Sound pressure level-=-Cooling-=-At medium fan speed","","dBA","41.0"]
["","Sound pressure level-=-Heating-=-At high fan speed","","dBA","45.0"]
["","Sound pressure level-=-Heating-=-At medium fan speed","","dBA","41.0"]
["","Sound pressure level-=-Cooling-=-At low fan speed","","dBA","36.0"]
["Sound power level","Sound power level-=-Cooling-=-At high fan speed","","dBA","61.0"]
["Sierpaneel","Sierpaneel-=-Afmetingen-=-Breedte","","mm","950"]
["Geluidsdrukniveau","Sound pressure level-=-Heating-=-At low fan speed","","dBA","36.0"]
["Sierpaneel","Sierpaneel-=-Afmetingen-=-Hoogte","","mm","65"]
["Uitblaaspaneel 2-=-Gewicht","kg","","","10.3"]
["Sierpaneel","Sierpaneel-=-Afmetingen-=-Diepte","","mm","950"]
["Uitblaaspaneel-=-Gewicht","kg","","","5.5"]
["Uitblaaspaneel 2","Uitblaaspaneel 2-=-Afmetingen-=-H","","mm","148"]
["","Uitblaaspaneel 2-=-Afmetingen-=-B","","mm","950"]
["","Uitblaaspaneel 2-=-Afmetingen-=-D","","mm","950"]
["Leidingaansluitingen","Leidingaansluitingen-=-Vloeistof-=-Buitendiameter","","mm","10"]
["Leidingaansluitingen","Piping connections-=-Gas-=-OD","","mm","15.90"]
["Uitblaaspaneel 3","Uitblaaspaneel 3-=-Afmetingen-=-B","","mm","950"]
["","Uitblaaspaneel 3-=-Afmetingen-=-H","","mm","106"]
["","Uitblaaspaneel 3-=-Afmetingen-=-D","","mm","950"]
["Uitblaaspaneel 3-=-Gewicht","kg","","","6.5"]
["Standaard-accessoires","Wire clamp material","","","7"]
["","Clamps","","","1"]
["","Insulation for fitting","","","2"]
["","Sealing pads","","","1"]
["Spanningsvorm","Spanningsvorm-=-Spanning","","","220-240/220"]
["","Spanningsvorm-=-Frequentie","","","50/60"]
["Stroom - 50Hz-=-Afzekerwaarde","A","","","6"]