{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","500"]
["","","","Breedte","mm","270"]
["","","","Diepte","mm","270"]
["Gewicht","Unit","","","kg","6.8"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Fluisterstil","kW","0.008"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Turbo-=-dB(A)","dBA","53"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Middelhoog-=-dB(A)","dBA","39"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Laag-=-dB(A)","dBA","29"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Fluisterstil-=-dB(A)","dBA","19"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Turbo-=-m³/u","m³/u","330"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Middelhoog-=-m³/u","m³/u","192"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Laag-=-m³/u","m³/u","120"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Fluisterstil-=-m³/u","m³/u","66"]
["Veiligheidsvoorzieningen","Onderdeel","","01","","Veiligheidsschakelaar (Werking stopt wanneer het deksel van de Streamer-unit open is)"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie-=-Hz","","","Hz","50/60"]
["","Spanningsvorm-=-Spanning-=-V","","","V AC","220-240/220-230"]
["Bedrijfsstroom","Werking luchtreiniging","","Turbo","A","0.32"]
["","","","Middelhoog","A","0.14"]
["","","","Laag","A","0.10"]
["","","","Fluisterstil","A","0.08"]