{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Behuizing","Kleur","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","700 (1)"]
["","","","Breedte","mm","270"]
["","","","Diepte","mm","270 (4)"]
["Gewicht","Unit","","","kg","9.5"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Fluisterstil","kW","0.007"]
["Bevochtiging","Opgenomen vermogen","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Fluisterstil","kW","0.011"]
["","Inhoud waterreservoir","","","l","2.7"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Turbo-=-dB(A)","dBA","53.0"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Middelhoog-=-dB(A)","dBA","39.0"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Laag-=-dB(A)","dBA","29.0"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Fluisterstil-=-dB(A)","dBA","19.0"]
["","Geluidsdrukniveau op 1 m-=-Bevochtiging","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Turbo-=-dB(A)","dBA","53.0"]
["","","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Middelhoog-=-dB(A)","dBA","39.0"]
["","","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Laag-=-dB(A)","dBA","33.0"]
["","","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Fluisterstil-=-dB(A)","dBA","25.0"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Turbo-=-m³/u","m³/u","330"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Middelhoog-=-m³/u","m³/u","192"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Laag-=-m³/u","m³/u","120"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Fluisterstil-=-m³/u","m³/u","54"]
["","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Turbo-=-m³/u","m³/u","330"]
["","","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Middelhoog-=-m³/u","m³/u","192"]
["","","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Laag-=-m³/u","m³/u","144"]
["","","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Fluisterstil-=-m³/u","m³/u","102"]
["Standaard-accessoires","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie-=-Hz","","","Hz","50/60"]
["","Spanningsvorm-=-Spanning-=-V","","","V AC","220-240/220-230"]
["Bedrijfsstroom","Werking luchtreiniging","","Turbo","A","0.50"]
["","","","Middelhoog","A","0.19"]
["","","","Laag","A","0.12"]
["","","","Fluisterstil","A","0.09"]
["","Bevochtiging","","Turbo","A","0.50"]
["","","","Middelhoog","A","0.20"]
["","","","Laag","A","0.15"]
["","","","Fluisterstil","A","0.13"]
["Opmerkingen","","","","","(1) - Alleen 3-fasig"]
["","","","","","(2) - Andere functie: Automatische herstartfunctie."]
["","","","","","(3) - Safety valve"]
["","","","","","(4) - Getest bij Ta DB/NB 14°C/13°C. Conform EN 16147."]