{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Laag-=-m³/u","m³/u","132"]
["","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Laag-=-m³/u","m³/u","132"]
["","","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Turbo-=-m³/u","m³/u","420"]
["","","","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Middelhoog-=-m³/u","m³/u","210"]
["Bevochtiging","Opgenomen vermogen","","L","kW","0.012"]
["Werking luchtreiniging","Opgenomen vermogen","","Fluisterstil","kW","0.008"]
["Bevochtiging","Inhoud waterreservoir","","","l","3.6"]
["Werking luchtreiniging","Opgenomen vermogen","","M","kW","0.016"]
["Bevochtiging","Opgenomen vermogen","","Fluisterstil","kW","0.011"]
["","","","M","kW","0.018"]
["Werking luchtreiniging","Opgenomen vermogen","","L","kW","0.010"]
["Bevochtiging","Opgenomen vermogen","","Turbo","kW","0.068"]
["Toepassing","","","","","Vloermodel"]
["Gewicht","Unit","","","kg","12.5"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.066"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Bevochtiging","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Fluisterstil-=-dB(A)","dBA","23"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Fluisterstil-=-m³/u","m³/u","60"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Bevochtiging","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Laag-=-dB(A)","dBA","27"]
["","","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Turbo-=-dB(A)","dBA","54"]
["Geschikt voor vloeroppervlakte","m²","","","","48, 96"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging","Ventilator--=-Luchthoeveelheid-=-Werking luchtreiniging-=-Turbo-=-m³/u","m³/u","420"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Fluisterstil-=-dB(A)","dBA","18"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Turbo-=-dB(A)","dBA","54"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Middelhoog-=-dB(A)","dBA","37"]
["","Geluidsdrukniveau op 1 m-=-Bevochtiging","","Geluidsdrukniveau op 1 m-=-Bevochtiging-=-Middelhoog-=-dB(A)","dBA","37"]
["","","","Geluidsdrukniveau op 1 m-=-Werking luchtreiniging-=-Laag-=-dB(A)","dBA","27"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Bevochtiging","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Middelhoog-=-m³/u","m³/u","210"]
["","","","Ventilator--=-Luchthoeveelheid-=-Bevochtiging-=-Fluisterstil-=-m³/u","m³/u","102"]
["Behuizing","Kleur","","","","Wit (N9. 0)"]
["Afmetingen","Unit","","Diepte","mm","287"]
["","","","Breedte","mm","395"]
["Type","","","","","Luchtbevochtiger en -reiniger"]
["Afmetingen","Unit","","Hoogte","mm","600"]
["CADR","m³/u","","","","375"]
["Stofvangmethode","","","","","Elektrostatisch HEPA-filter"]
["Deodorizing method","","","","","Flash streamer + ontgeurende katalysator"]
["Standaard-accessoires","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50/60"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240/220-230"]
["Voeding","Fase","","","","1~"]
["Voedingskabel","m","","","","2.0"]
["Opmerkingen","","","","","(1) - Omgezet naar NRCC-normen van testwaarden overeenkomstig JEM1467."]
["","","","","","(2) - De gedekte oppervlakte is geschikt voor het gebruiken van de unit met maximaal ventilatortoerental (HH). De gedekte oppervlakte geeft de ruimte aan waarin een bepaalde hoeveelheid stofdeeltjes in 30 minuten verwijderd kan worden."]
["","","","","","(3) - De geluidsniveaus zijn het gemiddelde van de waarden gemeten op 1 m afstand van de voorkant, linker- en rechterkant en achterkant van de unit. (Deze zijn gelijk aan de waarde in een echoloze ruimte)"]