{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B"]
["Afmetingen","Unit","","Hoogte","mm","990"]
["","","","Breedte","mm","940"]
["","","","Diepte","mm","320"]
["Gewicht","Unit","","","kg","67"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Werkingsbereik-=-Koelen","Werkingsbereik-=-Koelen-=- ","Werkingsbereik-=-Koelen-=- -=-Min.-=-°CDB","°C DB","-15"]
["","","","Werkingsbereik-=-Koelen-=- -=-Max.-=-°CDB","°C DB","50"]
["","Verwarmen","Werkingsbereik-=-Verwarmen-=- ","Werkingsbereik-=-Verwarmen-=- -=-Min.-=-°CWB","°CWB","-20"]
["","","","Werkingsbereik-=-Verwarmen-=- -=-Max.-=-°CWB","°CWB","15.5"]
["Geluidsvermogenniveau","Koelen","","","dBA","64"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dBA","48"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dBA","50"]
["","Geluidsdrukniveau op 1 m-=-Fluisterstille nachtstand","","Geluidsdrukniveau op 1 m-=-Fluisterstille nachtstand-=-Niveau 1-=-dB(A)","dBA","43"]
["Koelmiddel","Type","","","","R-32"]
["Koudemiddel","Koudemiddel-=-Inhoud-=-kg","","","kg","2.6"]
["Koelmiddel","GWP","","","","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.8"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","15.9"]
["Koelleidingmaten","Koelleidingmaten-=-Leidinglengte","Koelleidingmaten-=-Leidinglengte-=- ","Koelleidingmaten-=-Leidinglengte-=- -=-Max.-=-m","m","55"]
["","","Koelleidingmaten-=-Leidinglengte-=-Systeem","Koelleidingmaten-=-Leidinglengte-=-Systeem-=-Equivalent-=-m","m","75"]
["","","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot","Koelleidingmaten-=-Leidinglengte-=-Voorgevuld tot-=- -=-m","m","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding"]
["Koelleidingmaten","Koelleidingmaten-=-Hoogteverschil","Koelleidingmaten-=-Hoogteverschil-=- ","Koelleidingmaten-=-Hoogteverschil-=- -=-Max.-=-m","m","30.0"]
["","","Koelleidingmaten-=-Hoogteverschil-=-IU - IU","Koelleidingmaten-=-Hoogteverschil-=-IU - IU-=-Max.-=-m","m","0.5"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Spanningsvorm-=-Frequentie-=-Hz","","50/60"]
["","Spanningsvorm-=-Spanning","","Spanningsvorm-=-Spanning-=-V","","220-240"]