{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":16,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R"]
[]
[]
[]
[]
["","","","","","FTXM20R5V1B","FTXM20R2V1B","FTXM25R2V1B","FTXM25R5V1B","FTXM35R5V1B","FTXM35R2V1B","FTXM42R5V1B","FTXM42R2V1B","FTXM50R2V1B","FTXM60R2V1B","FTXM71R2V1B"]
["Puissance absorbée","Puissance absorbée-=-Chauffage","","Puissance absorbée-=-Chauffage-=-Nom.-=-kW","kW","0.023","0.023","0.022","0.022","0.027","0.027","0.038","0.038","0.032","0.035","0.06"]
["","Puissance absorbée-=-Rafraîchissement","","Puissance absorbée-=-Rafraîchissement-=-Nom.-=-kW","kW","0.029","0.029","0.025","0.025","0.030","0.030","0.034","0.034","0.03","0.032","0.054"]
["Niveau de puissance sonore","Niveau de puissance sonore-=-Chauffage-=-dBA","","","dBA","54","54","54","54","54","54","60","60","58","59","61"]
["Systèmes de contrôle","Infrared remote control","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Rafraîchissement","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Haut-=-m³/min","m³/min","10.5","10.5","10.5","10.5","11.3","11.3","11.9","11.9","15.8","16.7","16.9"]
["","","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Haut-=-m³/min","m³/min","9.3","9.3","9.8","9.8","9.8","9.8","12.4","12.4","15.8","16.5","17.7"]
["","","","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Bas-=-m³/min","m³/min","5.7","5.7","5.7","5.7","6.0","6.0","6.5","6.5","11.4","11.8","12.2"]
["","","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Bas-=-m³/min","m³/min","6.2","6.2","6.3","6.3","6.5","6.5","6.5","6.5","12","12.4","12.7"]
["Dimensions","Dimensions-=-Unité","","Dimensions-=-Unité-=-Largeur-=-mm","mm","778","778","778","778","778","778","778","778","998","998","998"]
["","","","Dimensions-=-Unité-=-Hauteur-=-mm","mm","295","295","295","295","295","295","295","295","299","299","299"]
["","","","Dimensions-=-Unité-=-Profondeur-=-mm","mm","272","272","272","272","272","272","272","272","292","292","292"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Faible niveau sonore de fonctionnement-=-dBA","dBA","20","20","20","20","20","20","21","21","31","33","34"]
["Ventilateur","Ventilateur-=-Débit d'air","Ventilateur-=-Débit d'air-=-Chauffage","Ventilateur-=-Débit d'air-=-Chauffage-=-Faible niveau sonore de fonctionnement-=-m³/min","m³/min","5.1","5.1","4.9","4.9","4.9","4.9","4.9","4.9","10.5","11.1","11.6"]
["","","Ventilateur-=-Débit d'air-=-Rafraîchissement","Ventilateur-=-Débit d'air-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement-=-m³/min","m³/min","4.3","4.3","4.1","4.1","4.2","4.2","4.3","4.3","8.3","9.1","10"]
["Niveau de pression sonore","Rafraîchissement","","Moyen","dBA","33","33","33","33","33","33","39","39","","42"]
["Ventilateur","Débit d'air","Chauffage","Moyen","m³/min","8.2","8.2","8","8","8.5","8.5","9.7","9.7","","15.2"]
["","","Rafraîchissement","Moyen","m³/min","7.5","7.5","7.6","7.6","7.8","7.8","9.0","9.0","","14.0"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Moyen-=-dBA","dBA","34","34","34","34","35","35","39","39","39","41","42"]
["","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Haut-=-dBA","dBA","41","41","41","41","45","45","45","45","44","46","47"]
["Poids","Unité","","","kg","10","10.0","10","10","10.0","10.0","10.0","10.0","","14.5"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Liquide","","Raccords de tuyauterie-=-Liquide-=-DE-=-mm","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Bas-=-dBA","dBA","25","25","25","25","29","29","30","30","36","37","38"]
["Raccords de tuyauterie","Gaz","","DE","mm","9.5","9.50","9.5","9.5","9.50","9.50","9.50","9.50","","12.7"]
["Niveau de pression sonore","Niveau de pression sonore-=-Rafraîchissement","","Niveau de pression sonore-=-Rafraîchissement-=-Faible niveau sonore de fonctionnement-=-dBA","dBA","19","19","19","19","19","19","21","21","27","30","32"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc","","Blanc"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Bas-=-dBA","dBA","26","26","27","27","28","28","29","29","34","36","37"]
["Niveau de puissance sonore","Niveau de puissance sonore-=-Rafraîchissement-=-dBA","","","dBA","57","57","57","57","58","58","60","60","58","60","60"]
["Niveau de pression sonore","Niveau de pression sonore-=-Chauffage","","Niveau de pression sonore-=-Chauffage-=-Haut-=-dBA","dBA","39","39","39","39","39","39","45","45","43","45","46"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Évacuation","","","","18","18","18","18","18","18","18","18","18","18","18"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","1","1","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1","1","1"]
["Alimentation électrique","Alimentation électrique-=-Nom","","","","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Alimentation électrique-=-Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["","Alimentation électrique-=-Fréquence","","Alimentation électrique-=-Fréquence-=-Hz","","50","50","50","50","50","50","50","50","50","50","50"]
["Caisson","Caisson-=-Couleur","","","","","","","","","","","","Blanc","","Blanc"]
["Poids","Poids-=-Unité-=-kg","","","kg","","","","","","","","","14.5","","14.5"]
["Ventil.","Ventil.-=-Débit d'air","Ventil.-=-Débit d'air-=-Refroidissement","Ventil.-=-Débit d'air-=-Refroidissement-=-Moyen-=-m³/min","m³/min","","","","","","","","","14","","15"]
["","","Ventil.-=-Débit d'air-=-Chauffage","Ventil.-=-Débit d'air-=-Chauffage-=-Moyen-=-m³/min","m³/min","","","","","","","","","14.2","","15.8"]
["Niveau de pression sonore","Niveau de pression sonore-=-Refroidissement","","Niveau de pression sonore-=-Refroidissement-=-Moyen-=-dBA","dBA","","","","","","","","","40","","43"]
["Raccords de tuyauterie","Raccords de tuyauterie-=-Gaz","","Raccords de tuyauterie-=-Gaz-=-DE-=-mm","mm","","","","","","","","","12.7","","15.9"]
["Systèmes de commande","Systèmes de commande-=-Télécommande câblée","","","","","","","","","","","","BRC073A1","","BRC073A1"]
["Accessoires standard","Silver particle filter","","","","","","","","","","","","1","1","1"]